|  |  |  |
| --- | --- | --- |
| undefined  **22** - ultimele 2 cifre ale aplicarii initiale  **0090**  **01234**/01.01.01 - Nr. Declaratie, se sterge acest comentariu | | |
| Manufacturer, address, logo: |  | |
| Authorized representative: |  | |
| Unique identification code of the product-type: |  | |
| Intended use/es: |  | |
| Harmonized standard: | **EN 1090-1+A2:2012; EN 1090-2:2018** | |
| Notified body: | **TÜV Thüringen e.V. Melchendorfer Straße 64, D-99096 Erfurt, NoBo 0090** | |
| Declared performances: | Geometric tolerances |  |
| Weldability |  |
|  | Fracture toughness |  |
|  | Reaction to fire | **Material classified Class A1** |
|  | Release of cadmium | **NPD** |
|  | Emission of radioactivity | **NPD** |
|  | Durability |  |
|  | Structural characteristics | **NPD** |
|  | Design | **NPD** |
|  | Manufacturing | **According to component specification CS\_34/2006 and EN 1090-2 EXC2** |
| Appropriate Technical Documentation and/or Specific Technical Documentation: |  | |
| The performance of the product identified above is in conformity with the set of declared performance/s.  This declaration of performance is issued, in accordance with Regulation (EU) No 305/2011, under the sole responsibility of the manufacturer identified above. | | |
| Signed for and on behalf of the manufacturer by:  Name\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Place\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_Date\_\_\_\_\_\_\_\_\_\_\_\_\_Signature\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ | | |